Addendum # 1 to RFP 1229W

BCT Building renovation

Post Request by: Henning Hansen

3/8/2012

1. AC units listed to be on the north side are on the south side.
2. Contractor shall be responsible for the removal and reinstallation of all of the Handicap door hardware.
3. Contractor shall arrange for the power to be disconnected and reconnected in corporation with Owner to allow for safe working conditions in that area.
4. The gas service line will need to be removed and reinstalled to accommodate the new siding.
5. One bathroom vent and water heater drain line will have to be removed and reinstalled.
6. Owner will allow for handicap ramp to be blocked to allow for construction.
7. Scrubs on west side will not be removed and they will need to be protected.
8. Commercial grade roll up doors will be allowed.

You must acknowledge this addendum be signing it below and attaching it to your proposal.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_